#
FRONT FLOOR COVERING REMOVAL/INSTALLATION [WGN]

id0917004620a2

1. Disconnect the negative battery cable.

2. Remove the front seats.

3. Remove the rear seat. (See REAR SEAT REMOVAL/INSTALLATION [WGN (4WD)].)

4. Remove the front scuff plates.

5. Remove the rear scuff plates.

6. Remove the console.

7. Remove the front side trims.

8. Remove the B-pillar lower trims.

9. Remove the lower anchor of the front seat belt installation bolts.

10. Remove the tire house trim.

11. Remove the fuel-filler lid opener bezel.

12. Remove the fasteners.

13. Remove the cap nuts.

14. Remove the clips.

15. Take the front floor covering off from the passenger-side door opening.

16. Install in the reverse order of removal.