#
TRAILING LINK REMOVAL/INSTALLATION [4WD]

id0214008020a2

  Caution

  • Performing the following procedures without first removing the ABS wheel-speed sensor may possibly cause an open circuit in the harness if it is pulled by mistake. Before performing the following procedures, remove the ABS wheel-speed sensor (axle side) and fix it to an appropriate place where the sensor will not be pulled by mistake while servicing the vehicle.

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

3. Inspect the rear wheel alignment.

(See REAR WHEEL ALIGNMENT.)

.

1 | ABS wheel-speed sensor
2 | Parking brake cable
3 | Bolt (shock absorber lower side)
4 | Bolt (trailing link front side) (See Bolt (Trailing Link Front Side) Removal Note.) (See Bolt (Trailing Link Front Side) Installation Note.)
5 | Bolt (Lateral link outer side) (See Bolt (Lateral Link Outer Side) Removal Note.) (See Bolt (Lateral Link Outer Side) Installation Note.)
6 | Toe link bracket
7 | Trailing link

## Bolt (Trailing Link Front Side) Removal Note

1. Support the trailing link with a jack.

  Caution

  • Removing the trailing link is dangerous. The trailing link could fall and cause serious injury or death. Verify that the jack securely supports the trailing link.

2. Remove the bolts (trailing link front side).

## Bolt (Lateral Link Outer Side) Removal Note

1. Loosen the bolt (lateral link inner side).

2. Remove the bolt (lateral link outer side).

## Bolt (Lateral Link Outer Side) Installation Note

1. Tighten the bolt (lateral link outer side).

2. Tighten the bolt (lateral link inner side).

Tightening torque

  86.2-116.6 N·m {8.80-11.88 kgf·m, 63.58-85.99 ft·lbf}

## Bolt (Trailing Link Front Side) Installation Note

1. Support the trailing link with a jack.

2. Tighten the bolts (trailing link front side).