#
FUEL TANK REMOVAL/INSTALLATION [L3 Turbo]

id0114b4801600

  Warning

  • Repairing a fuel tank that has not been properly steam-cleaned can be dangerous. Explosion or fire may cause death or serious injury. Always properly steam clean a fuel tank before repairing it.
  • Fuel line spills and leakage are dangerous. Fuel can ignite and cause serious injuries or death and damage. Fuel can also irritate skin and eyes. To prevent this, do not damage the sealing surface of the fuel pump unit when removing or installing.
  • A person charged with static electricity could cause a fire or explosion, resulting in death or serious injury. Before draining fuel, make sure to discharge static electricity by touching the vehicle body.

  Caution

  • Disconnecting/connecting the quick release connector without cleaning it may cause damage to the fuel pipe and quick release connector. Always clean the quick release connector joint area before disconnecting/connecting using a cloth or soft brush, and make sure that it is free of foreign material.

1. Level the vehicle.

2. Complete the "BEFORE SERVICE PRECAUTION". (See BEFORE SERVICE PRECAUTION [L3 Turbo].)

3. Remove the propeller shaft. (See PROPELLER SHAFT REMOVAL/INSTALLATION [A26MX-R].)

4. Remove the middle pipe. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L3 Turbo].)

5. Disconnect the negative battery cable.

6. Remove the fuel pump unit. (SeeFUEL PUMP UNIT REMOVAL/INSTALLATION [L3 Turbo].)

7. Siphon the fuel from the fuel tank.

8. Remove in the order indicated in the table.

9. Install in the reverse order of removal.

10. Complete the "AFTER SERVICE PRECAUTION". (See AFTER SERVICE PRECAUTION [L3 Turbo].)

.

1 | Joint hose
2 | Fuel tank
3 | Evaporative hose
4 | Fuel-filler pipe
5 | Air filter