#
SOLENOID VALVE REMOVAL/INSTALLATION (PRIMARY CONTROL VALVE BODY) [FS5A-EL]

id051721807800

1. Disconnect the negative battery cable.

2. Remove the under cover.

3. Drain the ATF.

4. Remove the oil pan.

5. Remove the primary control valve body. (See PRIMARY CONTROL VALVE BODY REMOVAL [FS5A-EL].)

6. Remove the solenoid valve(s).

7. Apply ATF to a new O-ring and install it on the solenoid valve.

8. Install the solenoid valve in the primary control valve body.

Tightening torque

  7.8-10.8 N·m
  {80-110 kgf·cm, 70-95.4 in·lbf}

9. Install the primary control valve body. (See PRIMARY CONTROL VALVE BODY REMOVAL [FS5A-EL].)

10. Install the oil pan. (See PRIMARY CONTROL VALVE BODY REMOVAL [FS5A-EL].)

11. Install the under cover.

12. Connect the negative battery cable.

13. Add ATF. (See AUTOMATIC TRANSAXLE FLUID (ATF) REPLACEMENT [FS5A-EL].)

14. Perform the mechanical system test. (See MECHANICAL SYSTEM TEST [FS5A-EL].)

15. Perform the road test. (See ROAD TEST [FS5A-EL].)