#
AUTOMATIC TRANSAXLE OUTLINE [FS5A-EL]

id051721101700
• The electronic control automatic transaxle with the FS5A-EL type 5-speed lockup function, merging advanced electrical and mechanical technologies, has been adopted.
• A manual mode shift control has been adopted.

  - The manual mode shift control is activated by moving the selector lever from the D to M range position.
  - The automatic shift system automatically shifts between 1GR and 5GR. The manual shift system allows for free gear position selection by manually operating the selector lever forward and back.

• The level gauge of the FS5A-EL type measures the ATF level on the differential side, and the ATF inspection procedure differs from the FN4A-EL type.