#
TRUNK SIDE UPPER TRIM REMOVAL/INSTALLATION [5HB]

id091700803202

1. Disconnect the negative battery cable. (LH only)

2. Remove the tire house trim.

3. Remove the rear seat remote lever.

4. Remove the screw.

5. Pull the trunk side upper trim toward you, then disengage clips A from the body.

6. Disconnect the cargo compartment light connector. (LH only)

7. Install in the reverse order of removal.