#
POWER OUTSIDE MIRROR INSPECTION

id091200807600

1. Disconnect the power outside mirror connector.

2. Apply battery positive voltage to the power outside mirror terminals and inspect the operation of the power outside mirror.

  • If there is any malfunction, replace the power outside mirror.

Mirror operation | Terminal
--- | ---
B+ | GND
Up | B | D
Down | D | B
Left | F | D
Right | D | F

3. Inspect for continuity between the power outside mirror heater terminals.

  • If there is any malfunction, replace the power outside mirror.