#
CYLINDER BLOCK (I) DISASSEMBLY [WITH DIESEL PARTICULATE FILTER]

id0110f3500600

1. Disassemble in the order indicated in the table.

1 | Flywheel (See Flywheel Disassembly Note)
2 | End plate
3 | Oil filter
4 | Oil cooler
5 | Oil pan (See Oil Pan Disassembly Note)
6 | Oil strainer
7 | Oil pan upper block (See Oil Pan Upper Block Disassembly Note)
8 | Rear cover (SeeRear Cover Disassembly Note)
9 | Oil pump (seeOil Pump Disassembly Note)
10 | Thermostat
11 | Water pump
12 | Oil pump cover
13 | Relief valve
14 | Outer rotor
15 | Oil pump body
16 | Oil pump plate

## Flywheel Disassembly Note

1. Hold the flywheel using the SST.

2. Loosen the bolts in two or three steps in the order shown.

## Oil Pan Disassembly Note

1. Remove the oil pan mounting bolts.

2. Remove the sealant from the bolt threads.

3. Screw an oil pan bolt into the weldnut to make a small gap between the cylinder block and the oil pan.

4. Remove the oil pan using the separator tool.

## Oil Pan Upper Block Disassembly Note

1. Loosen the oil pan upper block bolts in two or three steps in the order shown.

2. Remove the oil pan upper block

## Rear Cover Disassembly Note

1. Remove the oil seal using a screwdriver protected with a rag.

## Oil Pump Disassembly Note

1. Remove the oil seal using a screwdriver protected with a rag.