#
HVAC SPECIFICATIONS [FULL-AUTO AIR CONDITIONER]

id0700001003a1

Item | Specification
--- | ---
L3, L8, LF, L3 Turbo | MZR-CD (RF Turbo)
Heating capacity | (kW {kcal/h}) | 4.400 {3,784} | 5.120 {4,403}
Airflow volume (during heater operation) | Blower motor | (m3/h) | 310 (L.H.D.) 300 (R.H.D.) | 280 (L.H.D.) 270 (R.H.D.)
Electricity consumption (during heater operation) | Blower motor | (W) | 184 | ←
Cooling capacity | (kW {kcal/h}) | 4.200 {3,612} | ←
Airflow volume (during air conditioner operation) | Blower motor | (m3/h) | 460 | ←
Electricity consumption (during air conditioner operation) | Blower motor | (W) | 225 | ←
Magnetic clutch | (W) | 46 | 45
Fan type | Blower motor | Sirocco fan | ←
Refrigerant | Type | R-134a | ←
Regular amount (approx. quantity) | 470 {16.6} (L.H.D.) 430 {15.2} (R.H.D.) | ←
(g {oz})
A/C compressor | Type | Vane-rotary | ←
Discharge capacity | 120 {120, 4.06} | ←
(ml {cc, fl oz})
Max. allowable speed | 7,200 | 6,400
(rpm)
Lube oil | Type | ATMOS GU10 | ←
Sealed volume (approx. quantity) | 150 {150, 5.07} | ←
(ml {cc, fl oz})
Magnetic clutch clearance | 0.3-0.5 {0.012-0.019} | ←
(mm {in})
Condenser | Type | Multiflow (sub-cooling type) | ←
Radiated heat | (kW {kcal/h}) | 5.15 {4,429}: European (L.H.D.) specs. 5.96 {5,130}: Australian, General (L.H.D. R.H.D.), U.K. specs. | 5.15 {4,429}
Receiver/drier capacity | (ml {cc, fl oz}) | 180 {180, 6.08}: European (L.H.D.) specs. 190 {190, 6.42}: Australian, General (L.H.D. R.H.D.), U.K. specs. | 180 {180, 6.08}
Desiccant | Synthetic zeolite | ←
Expansion valve | Type | Block type | ←
Evaporator | Type | Double-tank drawn cup | ←
Refrigerant pressure switch | Type | Dual-pressure: L3 (General (R.H.D.), L8, LF (except General (L.H.D.) specs.) | ←
Operating pressure |  | ←
(MPa {kgf/cm2, psi})
Type | Triple-pressure: L3 (except General (R.H.D.) specs.), LF (General (L.H.D.) specs.), L3 Turbo | -
Operating pressure |
(MPa {kgf/cm2, psi})
Thermal protector | Type | Bimetallic (Indirect sensing type) | ←
Operating temperature |  |
(°C {°F})
Sensor | Solar radiation sensor | Photodiode | ←
Ambient temperature sensor | Thermistor | ←
Cabin temperature sensor
Evaporator temperature sensor
Water temperature sensor
Actuator | Air intake actuator | Sliding contact type | ←
Air mix actuator, airflow mode actuator | Potentiometer type | ←
Temperature control | Reheat full air mix type | ←