#
REFRIGERANT LINES REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

id0711008030d3

1. Remove the battery.

2. Discharge the refrigerant from the system.

3. Remove the washer tank.

4. Remove the air cleaner cover, air cleaner element and air cleaner case.

5. Remove the sedimentor.

6. Remove the No.3 engine mount.

7. Remove the water heater unit. (See WATER HEATER UNIT REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

8. Remove the shroud panel.

9. Remove the right splash shield.

  Caution

  • If moisture or foreign material enters the refrigeration cycle, cooling ability will be lowered and abnormal noise will occur. Always immediately plug all open fittings after removing any refrigeration cycle parts to keep moisture or foreign material out of the cycle.

10. Remove in the order indicated in the table. Do not allow compressor oil to spill.

11. Install in the reverse order of removal.

12. Perform the refrigerant system performance test.

.

1 | Cooler pipe No.1
2 | Cooler pipe No.2
3 | Cooler pipe No.3
4 | Cooler pipe No.4
5 | Cooler pipe No.5 (R.H.D. only)
6 | Cooler hose (HI)
7 | Cooler hose (LO)