GENERATOR DISASSEMBLY/ASSEMBLY [MZR-CD (RF Turbo)]

id0117f1800400

  Caution
  • Melt the solder quickly, otherwise the diodes (rectifier) and regulator will be damaged by excessive heat.

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

dpe117bw1005

1 | Front cover
2 | Pulley (See Pulley Disassembly/Assembly Note.)
3 | Rotor
4 | Bearing
5 | Stator coil
6 | Rectifier
7 | Brush holder
8 | Rear bracket

Pulley Disassembly/Assembly Note

1. Bore a hole in the generator bearing cover with a flathead screwdriver as shown in the figure and remove the generator bearing cover.

am5ezw00002409

2. Disassemble/assemble the pulley using the SST.

zmu117wa1

  Tightening torque

  60—85 N·m {6.1—8.7 kgf·m, 45—62 ft·lbf}