#
C-PILLAR TRIM REMOVAL/INSTALLATION [4SD, 5HB]

id0917004591a1

## 4SD

1. Remove the tire house trim.

2. Turn the seaming welt over.

3. Remove the cap using a fastener remover, and remove the bolt (with curtain air bag system).

4. Disengage clips A and clip B using a fastener remover.

5. Pull the C-pillar trim forward, then disengage hook C from the body, and remove the C-pillar trim.

6. Install in the reverse order of removal.

## 5HB

1. Remove the tire house trim.

2. Remove the trunk side upper trim

3. Turn the seaming welt over.

4. Remove the cap using a fastener remover the bolt. (with curtain air bag system)

5. Disengage clips A and pin B using a fastener remover.

6. Pull the C-pillar trim forward, then disengage the hook from the body.

7. Remove the rear center seat belt tongue from the C-pillar trim. (LH only)

8. Remove the C-pillar trim.

9. Install in the reverse order of removal.