CLUTCH PEDAL REMOVAL/INSTALLATION

id051000801200

1. Disconnect the negative battery cable.

2. Remove the battery and battery tray. (European (L.H.D.), General (L.H.D.) specs.)

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

5. Fully depress the clutch pedal, and verify that the engine starts.

am6zzw00007528

1 | Nut
2 | Clutch switch connector
3 | Clutch switch
4 | Starter interlock switch connector (General (L.H.D.) specs.)
5 | Starter interlock switch (General (L.H.D.) specs.) (See Starter Interlock Switch Installation Note.)
6 | Nut
7 | E-clip
8 | Pin
9 | Bushing
10 | Nut
11 | Push rod
12 | Clevis
13 | Pedal pad
14 | Clutch pedal

Starter Interlock Switch Installation Note

1. After installing the clutch pedal, adjust/inspect the clutch pedal. (See CLUTCH PEDAL ADJUSTMENT.)(See CLUTCH PEDAL INSPECTION.)

2. Insert the new starter interlock switch into the pedal bracket hole in the direction indicated by arrow A.

3. Slide the starter interlock switch pressing it in the direction indicated by arrow B until it is locked.

4. Fully depress the clutch pedal in the direction of arrow C, and verify that a click sound from the starter interlock switch is heard.

am6zzw00007529