#
BATTERY RECHARGING [MZR-CD (RF Turbo)]

id0117f1800700

  Warning

  • Keep all flames away from the battery, otherwise evaporated gas from the battery fluid may catch fire, and cause serious injury.
  • Remove the battery filler caps when recharging to prevent battery deformation or damage.

  Caution

  • Do not quick charge for more than 30 min. It will damage the battery.

1. Remove the battery and then place it in a pan of water.

2. Connect a battery charger to the battery and adjust the charging current as follows.

Battery slow charge current

  95D31L (64): 6.5-8.0 A
  115D31L (70): 7.0-8.5 A

Battery quick charge current [30 min.]

  95D31L (64): 40 A
  115D31L (70): 45 A

3. After the battery is recharged, verify that the voltage is within the specification and remains at the same value for 1 h or more after the recharging was completed.

  • If not within the specification, replace the battery.

Standard voltage

  12.4 V or more