#
TRANSAXLE FLUID TEMPERATURE (TFT) SENSOR INSPECTION [JA5AX-EL]

id051705801000

1. Disconnect the terminal component No.2 connector.

2. Remove the oil dipstick.

3. Insert the thermistor probe into the filler tube.

4. Start the engine.

5. Measure resistance between the terminals G and H.

  • If not as specified, replace the TFT sensor. (See AUTOMATIC TRANSAXLE AND TRANSFER REMOVAL/INSTALLATION [JA5AX-EL].) (See Automatic Transaxle Workshop Manual JA5A-EL.)

Transaxle fluid temperature (TFT) sensor

ATF temperature (°C {°F}) | Resistance (kilohm)
--- | ---
-20 {-4} | 15.87-17.54
0 {32} | 5.73-6.33
20 {68} | 2.38-2.63
40 {104} | 1.10-1.22
60 {140} | 0.56-0.62
80 {176} | 0.31-0.34
100 {212} | 0.18-0.20
120 {248} | 0.11-0.12
130 {266} | 0.09-0.10

6. Connect the terminal component No.2 connector.