#
EGR VALVE REMOVAL/INSTALLATION [L8, LF, L3]

id0116a4801000

1. Disconnect the negative battery cable.

2. Disconnect the EGR valve connector.

3. Remove in the order indicated in the table.

1 | Water hose (See Water Hose Removal Note.)
2 | EGR valve (See EGR Valve Removal Note.)

4. Install in the reverse order of removal.

## Water Hose Removal Note

• Drain the engine coolant. (See ENGINE COOLANT REPLACEMENT [L8, LF, L3, L3 Turbo].)

## EGR Valve Removal Note

1. Remove the air hose. (See INTAKE AIR SYSTEM REMOVAL/INSTALLATION [L8, LF, L3].)

2. Remove the upper radiator hose. (See RADIATOR REMOVAL/INSTALLATION [L8, LF, L3].)