#
WASHER FLUID-LEVEL SENSOR REMOVAL/INSTALLATION

id091900801800

1. Disconnect the negative battery cable.

2. Remove the washer tank. (See WASHER TANK REMOVAL/INSTALLATION.)

3. Remove the headlight cleaner motor. (See HEADLIGHT CLEANER MOTOR REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

1 | Connector
2 | Washer fluid-level sensor
3 | Grommet

5. Install in the reverse order of removal.