#
COOLING FAN MOTOR REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

id0112f1801900

  Warning

  • Remove and install all parts when the engine is cold, otherwise they can cause severe burns or serious injury.

1. Disconnect the negative battery cable.

2. Remove the shroud panel. (See SHROUD PANEL REMOVAL/INSTALLATION.)

3. Remove the cooler pipe stay. (See CONDENSER REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

1 | Cooling fan motor connectors
2 | Wiring harness
3 | Coolant reserve tank hose
4 | Cooling fan component
5 | Cooling fan No.1
6 | Cooling fan No.2
7 | Cooling fan motor No.1
8 | Cooling fan motor No.2