#
LIFTGATE SIDE TRIM REMOVAL/INSTALLATION [5HB]

id091700803702

1. Remove the liftgate upper trim.

2. Position the strap hanger as shown in the figure.

3. Pull the liftgate side trim toward you, then disengage clips A, pin B and the strap hanger from the body and pin B, hook C, D from the liftgate lower trim.

4. Remove the liftgate side trim.

5. Remove the hanger strap from the liftgate side trim.

6. Install in the reverse order of removal.