#
ENGINE DISASSEMBLY/ASSEMBLY [L8, LF, L3]

id0110a1800500

1. Disconnect the engine and transaxle. (See AUTOMATIC TRANSAXLE AND TRANSFER REMOVAL/INSTALLATION [JA5AX-EL].) (See MANUAL TRANSAXLE REMOVAL/INSTALLATION [G35M-R].) (See MANUAL TRANSAXLE REMOVAL/INSTALLATION [G66M-R].) (See AUTOMATIC TRANSAXLE REMOVAL/INSTALLATION [FS5A-EL].)

2. Remove the intake-air system. (See INTAKE AIR SYSTEM REMOVAL/INSTALLATION [L8, LF, L3].)

3. Remove the exhaust system. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L8, LF, L3 2WD].) (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L3 4WD].)

4. Remove the generator.

5. Remove the CKP sensor. (See CRANKSHAFT POSITION (CKP) SENSOR REMOVAL/INSTALLATION [L8, LF, L3].)

6. Assemble in the reverse order of disassembly.