#
SLIDE MOTOR INSPECTION

id091300800900

1. Disconnect the slide motor connector.

2. Inspect the slide motor operation when B+ is applied to the terminals as shown.

  • If not as specified, replace the seat cushion frame.

Motor operation | Connection
--- | ---
B+ | GND
Forward | 1A (1C) | 1C (1A)
Backward | 1C (1A) | 1A (1C)

3. Connect battery positive voltage to front tilt motor terminal 2A and connect terminal 2B to ground.

4. Operate the front tilt motor and measure the voltage at terminals 2A and 2B.

  • If there is any malfunction, replace the seat cushion frame.