#
EVAPORATIVE EMISSION (EVAP) CONTROL SYSTEM REMOVAL/INSTALLATION [L3 Turbo]

id0116b4736300

## Engine Compartment Side

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

1 | Purge solenoid valve (See Purge Solenoid Valve Installation Note.)
2 | Check valve
3 | PCV valve (See Positive Crankcase Ventilation (PCV) Valve Removal Note.)

## Positive Crankcase Ventilation (PCV) Valve Removal Note

1. Remove the intake manifold. (See INTAKE AIR SYSTEM REMOVAL/INSTALLATION [L3 Turbo].)

2. Remove the PCV valve.

## Purge Solenoid Valve Installation Note

1. Install the purge solenoid valve.

2. Fit the vacuum hose (purge solenoid valve) onto the respective fittings, and install clamps as shown.

## Fuel Tank Side

1. Raise the rear of the vehicle and support it with safety stands.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

.

1 | Protector
2 | Insulator
3 | Evaporative hose (See QUICK RELEASE CONNECTOR REMOVAL/INSTALLATION [L3 Turbo])
4 | Charcoal canister