#
DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)]

id0415008010a8

  Caution

  • When replacing the DSC HU/CM, configuration procedure must be done before removing the DSC HU/CM. If configuration is not completed before removing the DSC HU/CM, DTC B2477 will be detected.
  • The internal parts of the DSC HU/CM could be damaged if dropped. Be careful not to drop the DSC HU/CM. Replace the DSC HU/CM if it is subjected to an impact.

1. Configurate the DSC HU/CM (when only replacing it).(See DSC HU/CM CONFIGURATION.)

2. Remove the battery, battery tray and battery tray bracket. (See BATTERY REMOVAL/INSTALLATION [L8, LF, L3, L3 Turbo].) (See BATTERY REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

3. Remove the under cover.

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

.

1 | Connector (See Connector Removal Note) (See Connector Installation Note)
2 | Brake pipe
3 | DSC HU/CM and Bracket (See DSC HU/CM and Bracket Removal/Installation Note)
4 | Bracket
5 | DSC HU/CM

## Connector Removal Note

1. Release the lock lever to unlock it.

2. Remove the connector.

## Brake Pipe Removal Note

1. Mark the brake pipe connecting positions before removal for reference during installation.

## DSC HU/CM and Bracket Removal/Installation Note

1. When removing/installing the DSC HU/CM from/to the vehicle, attach a strip of tape on the DSC HU/CM connector to prevent brake fluid from entering.

## Brake Pipe Installation Note

1. When installing the brake pipe, align the marks made before removal with the DSC HU/CM as shown in the figure.

## Connector Installation Note

1. Verify that the connection part and waterproof packing are free of foreign material, then connect the connector.

2. Verify that the lock lever is completely pushed in.