#
ABS (ABS/TCS) HU/CM REMOVAL/INSTALLATION [MTX]

id0413008025a3

  Caution

  • When replacing the ABS (ABS/TCS) HU/CM, the configuration procedure must be done before removing the ABS (ABS/TCS) HU/CM. If the configuration is not completed before removing the ABS (ABS/TCS) HU/CM, ABS (ABS/TCS) will not work properly after installation of the ABS (ABS/TCS) HU/CM.
  • The internal parts of the ABS (ABS/TCS) HU/CM could be damaged if dropped. Be careful not to drop the ABS (ABS/TCS) HU/CM. Replace the ABS (ABS/TCS) HU/CM if it is subjected to an impact.

1. Configurate the ABS (ABS/TCS) HU/CM (only when replacing it). (See ABS (ABS/TCS) HU/CM CONFIGURATION.)

2. Remove the battery, battery tray and battery tray bracket. (See BATTERY REMOVAL/INSTALLATION [L8, LF, L3, L3 Turbo].) (See BATTERY REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

3. Remove the under cover.

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

1 | Connector (See Connector Removal Note) (See Connector Installation Note)
2 | Brake pipe (See Brake Pipe Removal Note) (See Brake Pipe Installation Note)
3 | ABS (ABS/TCS) HU/CM (See ABS (ABS/TCS) HU/CM Removal/Installation Note)
4 | Stud

## Connector Removal Note

1. Release the lock lever to unlock it.

2. Remove the connector.

## Brake Pipe Removal Note

1. Mark the brake pipe connecting positions before removal for reference during installation.

## ABS (ABS/TCS) HU/CM Removal/Installation Note

1. When removing/installing the ABS (ABS/TCS) HU/CM from/to the vehicle, attach a strip of protective tape on the ABS (ABS/TCS) HU/CM connector to prevent brake fluid from entering.

## Brake Pipe Installation Note

1. When installing the brake pipe, align the marks made before removal with the ABS (ABS/TCS) HU/CM as shown in the figure.

## Connector Installation Note

1. Verify that the lock lever of the harness connector is securely locked.