#
REAR DIFFERENTIAL REMOVAL/INSTALLATION [L3 Turbo]

id0314a4800400

1. Drain the rear differential oil into a container.

2. Remove the after silencer, presilencer, and catalytic converter. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L3 Turbo].)

3. Remove the propeller shaft. (See PROPELLER SHAFT REMOVAL/INSTALLATION [A26MX-R].)

4. Remove the rear drive shaft. (See REAR DRIVE SHAFT REMOVAL/INSTALLATION.)

5. Remove in the order indicated in the table.

6. Install in the reverse order of removal.

7. Add the specified rear differential oil.

1 | Differential oil temperature sensor connector
2 | 4WD solenoid connector
3 | Coupling component and rear differential component (See Coupling Component and Rear Differential Component Removal/installation Note)
4 | Rear differential bracket
5 | Coupling component (See COUPLING COMPONENT REMOVAL/INSTALLATION [L3 Turbo])
6 | Rear differential

## Coupling Component and Rear Differential Component Removal/installation Note

  Warning

  • Make sure that the coupling component and rear differential component are securely supported by the jack. If the coupling component and rear differential component fall, it could cause death, serious injury, or vehicle damage.

1. Make sure that the coupling component and rear differential component are securely supported by the jack, and remove/install the component by operating the jack gradually.