#
DOOR GARNISH REMOVAL

id091600801300

1. Cut the double-sided adhesive tape using a razor.

  Warning

  • Using a razor with bare hands can cause injury. Always wear gloves when using a razor.

  Note

  • The side protector is installed with double-sided adhesive tape. If the side protector is difficult to remove, soften the double-sided adhesive tape using a hot air blower.

2. Remove the clip A.

3. Pull the door garnish outward, then remove it.