#
CIGARETTE LIGHTER REMOVAL/INSTALLATION

id092000803100

1. Disconnect the negative battery cable.

2. Remove the console. (See CONSOLE REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Cigarette lighter plug
2 | Connector
3 | Socket (See Socket Removal Note)
4 | Ring (See Ring Removal Note)

4. Install in the reverse order of removal.

## Socket Removal Note

1. Insert a tape-wrapped screwdriver into the socket hole, then press against the ring protrusion to lift the socket toward you.

2. As shown in the figure, lift out the socket until the ring protrusion locks into the lower socket hole.

3. Remove the boot panel.

4. Front behind the boot panel, slide a tape-wrapped screwdriver in between the socket and the ring protrusion.

5. While twisting the ring protrusion with the screwdriver, push out and remove the socket.

## Ring Removal Note

1. Pull the ring forward while compressing the hooks.