#
ON-BOARD DIAGNOSTIC FUNCTION

id0702a2100300

## Present Failure Indication Mode

• In present failure indication mode, present failures in the control system circuits (open, short circuits) are detected, and the flashing of the rear defroster indicator light on the climate control unit indicates the DTCs shown in the table below.

## Past Failure Indication Mode

• In past failure indication mode, past failures (intermittent problems) in the input sensor circuits (open, short circuits) are stored, and the flashing of the rear defroster indicator light on the climate control unit indicates the DTCs shown in the table below. Erase DTCs from the memory after failures have been corrected so they are not maintained as past failures.

Diagnostic trouble codes

DTC No. | Indicator pattern | Diagnosed circuit | Detected condition | Memo rized
--- | --- | --- | --- | ---
02 |  | Solar radiation sensor (present) | Open circuit in solar radiation sensor circuit Short circuit in solar radiation sensor circuit (terminal B side only) | No
06 |  | Cabin temperature sensor (present) | Open/short circuit is in cabin temperature sensor circuit | No
07 |  | Cabin temperature sensor (past) | Cabin temperature sensor circuit is entered fail-safe mode at least once | Yes
10 |  | Evaporator temperature sensor (present) | Open/short circuit is in evaporator temperature sensor circuit | No
11 |  | Evaporator temperature sensor (past) | Evaporator temperature sensor circuit is entered fail-safe mode at least once | Yes
12 |  | Ambient temperature sensor (present) | Open/short circuit is in Ambient temperature sensor circuit | No
13 |  | Ambient temperature sensor (past) | Ambient temperature sensor circuit is entered fail-safe mode at least once | Yes
14 |  | Water temperature sensor (present) | Open/short circuit is in Water temperature sensor circuit | No
15 |  | Water temperature sensor (past) | Water temperature sensor circuit is entered fail-safe mode at least once | Yes
18 |  | Air mix actuator (potentiometer) (present) | Open/short circuit is in air mix actuator (potentiometer) circuit | No
19 |  | Air mix actuator (potentiometer) (past) | Air mix actuator (potentiometer) circuit is entered fail-safe mode at least once | Yes
21 |  | Airflow mode actuator (potentiometer) (present) | Open/short circuit is in airflow mode actuator (potentiometer) circuit | No
22 |  | Airflow mode actuator (potentiometer) (past) | Airflow mode actuator (potentiometer) circuit is entered fail-safe mode at least once | Yes
58 |  | Air mix actuator (motor lock) (past) | Air mix actuator circuit is entered fail-safe mode at least once | Yes
59 |  | Airflow mode actuator (motor lock) (past) | Airflow mode actuator circuit is entered fail-safe mode at least once | Yes

## Output Device Operation Check Mode

• In the output device operation check mode, the climate control unit forces all the output system actuation devices to operate regardless of the input system. The displays change and the switch indicator lights illuminate automatically according to the actuator operated.
• Inspect visually, listen for operation sound, and place hands over air discharge outlets to check for correct operating conditions and to locate the malfunctioning system.

Output device operation check table

Step | Operating device | Operating conditions | Moni tor* | Other device conditions
--- | --- | --- | --- | ---
1 | Blower motor speed |  | 1 | • Air mix actuator operation - 50% • Airflow mode actuator operation - VENT • Air intake actuator operation - FRESH • A/C compressor operation - ON
2 | Air mix actuator operation |  | 21.0 | • Blower motor speed - 3rd • Airflow mode actuator operation - VENT • Air intake actuator operation - FRESH • A/C compressor operation - ON
20.5
20.0
3 | Airflow mode actuator operation |  | 3 | • Blower motor speed - 3rd • Air mix actuator operation - 50% • Air intake actuator operation - FRESH • A/C compressor operation - ON
4 | Air intake actuator operation |  | 4 | • Blower motor speed - 3rd • Air mix actuator operation - 0% • Airflow mode actuator operation - VENT
A/C compressor operation |

  * :
Shown on the information display according to step.