#
DTC B2386

id0902b2844600

DTC B2386 | Discharge headlight illumination malfunction
DETECTION CONDITION | Warning • Incorrect servicing of the discharge headlight control module could result in electrical shock. Before servicing the discharge headlight control module, always refer to "Discharge headlight service warnings". (See DISCHARGE HEADLIGHT SERVICE WARNINGS) • Discharge headlight does not illuminate though preparation has been completed.
POSSIBLE CAUSE | • Discharge headlight bulb malfunction • Ignitor in front combination light is malfunctioning.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Are DTCs B2388 and/or B2389 indicated? | Yes | Replace discharge headlight bulb. (See HEADLIGHT BULB REMOVAL/INSTALLATION)
No | Ignitor in front combination light may be malfunctioning. Replace front combination light. (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION)