#
LCD UNIT CONSTRUCTION/OPERATION

id092000108400
• An LCD unit, located in the upper-center part of the dashboard to improve visibility, has been adopted.
• A pop-up LCD, controlled by an [OPEN/CLOSE] switch, has been adopted.
• The angle of the display screen can be adjusted in stages using the [TILT] switch.
• The audio, DIS and A/C information display is located on the lower portion of the unit. (See DRIVE INFORMATION SYSTEM STRUCTURAL VIEW.)

.

1 | LCD unit
2 | Open
3 | Close
4 | LCD for car-navigation system
5 | Information display

## Terminal Layout and Signals

Terminal | Signals
--- | ---
24-pin connector
| 1A | Video (B)
1B | Video (G)
1C | Video (composite sync)
1D | Video (R)
1E | Video GND
1F | -
1G | Shield GND
1H | -
1I | Monitor serial output
1J | -
1K | Monitor serial input
1L | -
1M | Control illumination
1N | -
1O | ACC
1P | GND
1Q | B+
1R | -
1S | Shield GND
1T | R-range
1U | UART2
1V | Illumination
1W | UART1
1X | -

Terminal | Signals
--- | ---
6-pin connector
| 2A | Remote-data
2B | Power
2D | Shield GND
2F | -
2G | GND
2H | Illumination

Terminal | Signal
--- | ---
1-pin connector
| 3A | GND