#
ELECTRICAL FAN CONTROL OPERATION [L8, LF, L3]

id0140a5104000

## Except for European (L.H.D. U.K.) L8, LF and Australian LF specs.

ON: Energized
OFF: De-energized

Condition | PCM terminal 1M | PCM terminal 1N*1/Not applicable*2 | PCM terminal 1R | Operation condition
--- | --- | --- | --- | ---
Cooling fan motor No. 1 | Cooling fan motor No. 2
Stopped | Stopped | OFF | OFF | OFF | A/C: OFF ECT: below 100 °C [212 °F]
Low speed | Low speed | ON | ON | OFF | A/C: OFF ECT: 100-108 °C [212-226 °F]
High speed | High speed | ON | ON | ON | A/C: OFF ECT: above 108 °C [226 °F]
Low speed | Low speed | ON | ON | OFF | A/C: ON (middle switch OFF) ECT: below 108 °C [226 °F]
High speed | Middle speed*3/ High speed*4 | ON | OFF*3/ON*4 | ON*3/OFF*4 | A/C: ON (middle switch ON) ECT: below 108 °C [226 °F]
High speed | High speed | ON | ON | ON | A/C: ON ECT: above 108 °C [226 °F]

  *1 :
Intensely hot area or General specs.
  *2 :
Except for intensely hot area and exsept for General specs.
  *3 :
Intensely for hot area and General (L.H.D.) specs.
  *4 :
Except for Intensely for hot area and General (L.H.D.) specs.

.

1 | Except for intensely hot area
2 | Intensely hot area
3 | Cooling fan relay No. 1
4 | Cooling fan relay No. 2
5 | Cooling fan relay No. 3
6 | Cooling fan relay No. 4
7 | Cooling fan motor No. 1
8 | Cooling fan motor No. 2

## European (L.H.D. U.K.) L8, LF and Australian LF specs.

• The PCM energized the cooling fan relay No. 1 and No. 2 except all of following condition are met.

  - ECT: below 100 °C [176 °F]
  - A/C: OFF

1 | Cooling fan relay No. 1
2 | Cooling fan relay No. 2
3 | Cooling fan motor No. 1
4 | Cooling fan motor No. 2