#
BEFORE REPAIR PROCEDURE [L8, LF, L3]

id0114b1802000

  Warning

  • Fuel vapor is hazardous. It can easily ignite, causing serious injury and damage. Always keep sparks and flames away from fuel.
  • Fuel line spills and leakage are dangerous. Fuel can ignite and cause serious injuries or death and damage. Fuel can also irritate skin and eyes. To prevent this, always complete the following "Fuel Line Safety Procedure".
  • A person charged with static electricity could cause a fire or explosion, resulting in death or serious injury. Before performing work on the fuel system, discharge static electricity by touching the vehicle body.

## Fuel Line Safety Procedure

  Note

  • Fuel in the fuel system is under high pressure also when the engine is not running.

1. Remove the fuel-filler cap and release the pressure in the fuel tank.

2. Remove the fuel pump relay.

3. Start the engine.

4. After the engine stalls, crank the engine several times.

5. Turn the ignition switch to LOCK position.

6. Install the fuel pump relay.