#
DTC P0072 [MZR-CD (RF Turbo)]

id0102f1117200

DTC P0072 | Exhaust gas pressure correction temperature sensor circuit low input
--- | ---
DETECTION CONDITION | • The PCM monitors the input signal from the exhaust gas pressure correction temperature sensor. If the voltage from the exhaust gas pressure correction temperature sensor is less than 0.09 V, the PCM determines that there is a malfunction in the exhaust gas pressure correction temperature sensor circuit. Diagnostic support note • The MIL illuminates if the PCM detects the above malfunction condition in the first drive cycle. • FREEZE FRAME DATA is available. • The DTC is stored in the PCM memory.
POSSIBLE CAUSE | • Exhaust gas pressure correction temperature sensor malfunction • Connector or terminal malfunction • Short to ground in wiring harness between exhaust gas pressure correction temperature sensor terminal A and PCM terminal 58 • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related service repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | VERIFY CURRENT SIGNAL STATUS: IS CONCERN INTERMITTENT OR CONSTANT? • Connect the WDS or equivalent to the DLC-2. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the same DTC present? | Yes | Go to the next step.
No | Intermittent concern exists. Perform the "INTERMITTENT CONCERN TROUBLESHOOTING". (See INTERMITTENT CONCERN TROUBLESHOOTING [MZR-CD (RF Turbo)].)
4 | INSPECT EXHAUST GAS PRESSURE CORRECTION TEMPERATURE SENSOR CONNECTOR FOR POOR CONNECTION • Turn the engine switch off. • Disconnect the exhaust gas pressure correction temperature sensor connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 8.
No | Go to the next step.
5 | INSPECT EXHAUST GAS PRESSURE CORRECTION TEMPERATURE SENSOR SIGNAL CIRCUIT FOR SHORT TO GROUND • Turn the engine switch off. • Disconnect the exhaust gas pressure correction temperature sensor connector. • Inspect for continuity between exhaust gas pressure correction temperature sensor terminal A (wiring harness-side) and body ground. • Is there continuity? | Yes | Repair or replace the wiring harness for a possible short to ground, then go to Step 8.
No | Go to the next step.
6 | INSPECT EXHAUST GAS PRESSURE CORRECTION TEMPERATURE SENSOR • Inspect the exhaust gas pressure correction temperature sensor. (See EXHAUST GAS PRESSURE CORRECTION TEMPERATURE SENSOR INSPECTION [MZR-CD (RF Turbo)].) • Is there any malfunction? | Yes | Replace the exhaust gas pressure correction temperature sensor, then go to Step 8. (See EXHAUST GAS PRESSURE SENSOR/EXHAUST GAS PRESSURE CORRECTION TEMPERATURE SENSOR REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to the next step.
7 | INSPECT PCM CONNECTOR FOR POOR CONNECTION • Turn the engine switch off. • Disconnect the PCM connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to the next step.
No | Go to the next step.
8 | VERIFY TROUBLESHOOTING OF DTC P0072 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the same DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to the next step.
9 | VERIFY AFTER REPAIR PROCEDURE • Perform the Repair Verification Drive Mode. (See OBD DRIVE MODE [MZR-CD (RF Turbo)].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [MZR-CD (RF Turbo)].)
No | DTC troubleshooting completed.