#
NO.6 RECEPTION FREQUENCY OF RADIO SLIPS

id0903a1804800

## Possible cause

• Audio unit malfunction
• Electronic jamming from outside, or inferior condition of broadcasting station radio wave

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Push SEEK button and check if desired broadcasting station is tuned. • Is it okay? | Yes | Go to the Step 3.
No | Go to the next step.
2 | • Check if other broadcasting station is received at certain place when indication of reception frequency stays. • Is other station received? Note • When you receive weak signal from one broadcasting station and come close to broadcasting antenna which emits strong signal, broadcasting with strong signal is sometimes received. | Yes | Go to the next step.
No | Replace audio unit. (SeeCENTER PANEL MODULE REMOVAL/INSTALLATION.) (SeeCENTER PANEL MODULE DISASSEMBLY/ASSEMBLY.) (SeeAUDIO UNIT DISASSEMBLY/ASSEMBLY.)
3 | • Compare reception with other audio unit on same model (model/unit) under same problem conditions. • Is reception equivalent between customers unit and compared unit? | Yes | Troubleshooting completed (Audio unit is normal).
No | Replace audio unit. (SeeCENTER PANEL MODULE REMOVAL/INSTALLATION.) (SeeCENTER PANEL MODULE DISASSEMBLY/ASSEMBLY.) (SeeAUDIO UNIT DISASSEMBLY/ASSEMBLY.)