#
TRANSAXLE OIL INSPECTION [G35M-R]

id0515b1800000

1. Park the vehicle on level ground.

2. Remove the oil level plug and washer.

3. Verify that the oil is near the brim of the plug port.

  • If the oil level is lower than the low level, add the specified amount and type of oil through the oil level plug hole.

Manual transaxle oil [G35M-R]

  Grade: API Service GL-4 or GL-5
  Viscosity (all-season): SAE 75W-90
  Viscosity (above 10 °C {50 °F}): SAE 80W-90

4. Install a new washer and the oil level plug.

Tightening torque

  39-59 N·m {4.0-6.0 kgf·m, 29-43 ft·lbf}