#
EVAPORATOR TEMPERATURE SENSOR INSPECTION

id074000801200

1. Turn the AUTO switch on.

2. Set the temperature control at MAX COLD (Turn the left).

3. Turn the A/C switch.

4. Set the RECIRCULATE mode.

5. Close all doors and windows.

6. Wait for 5 min.

7. Remove the glove compartment.

8. Disconnect the evaporator temperature sensor.

9. Measure the temperature at the blower inlet.

10. Measure the resistance between terminals of the evaporator temperature sensor.

  • If the resistance is not as shown in the graph, replace the evaporator temperature sensor.