#
REAR DOOR REMOVAL/INSTALLATION

id091100800300

  Warning

  • Handling the side air bag sensor improperly can accidentally operate (deploy) the side air bag module, which may seriously injure you. Read the service warnings and cautions before handling the side air bag sensor. (See SERVICE WARNINGS.) (See SERVICE CAUTIONS.)

  Note

  • The side air bag sensor is located in the B-pillar.

1. Disconnect the negative battery cable.

2. To remove the checker, turn the rear door speaker. (See REAR DOOR SPEAKER REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Connector
2 | Rear door hinge
3 | Rear door
4 | Checker

4. Install in the reverse order of removal.

5. Adjust the rear door. (See DOOR ADJUSTMENT.)