#
NO.13 NO KICKDOWN [JA5AX-EL]

id050305801800

13 | No kickdown
DESCRIPTION | • Does not downshift when accelerator pedal fully depressed within kickdown range.
POSSIBLE CAUSE | • If transaxle does not downshift though shifting is normal, malfunction is in TP sensor circuit (including sensor ground, sensor harness and connector). Note • Before following troubleshooting steps, make sure that Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.