ENGINE MOUNTING/DISMOUNTING

id011000507000

Installation

1. Install the SST (arms) to the four positions as shown in the figure and temporarily tighten the bolts (Part No.: 9YA20-1003) or M10 × 1.5T length 90 mm {3.55 in}.

b3e0110w127

2. Install the SSTs (bolts, nuts, hook, and plate) to the four positions as shown in the figure.

c3u0110e001

3. Install the SST (bolts, nuts, hook, and plate) set in Step 2 to the SST (arms and bolts) set in Step 1.

4. Adjust the bolts so that approx. 20 mm {0.79 in}of thread is exposed from the side of the plate.

5. Adjust the bolts and nuts so that the plate and arms are parallel.

6. Install the engine to the SST (engine stand).

e6u110zeb040

7. Remove the oil drain plug and drain the engine oil.

8. Replace the gasket with a new one and install the oil pan drain plug.

  Tightening torque

  30—41 N·m {3.1—4.1 kgf·m, 23—30 ft·lbf}

Removal

1. Remove in the reverse order of installation.