#
WINDSHIELD WASHER NOZZLE REMOVAL/INSTALLATION

id091900476300

1. Remove the bonnet insulator. (See BONNET REMOVAL/INSTALLATION [EXCEPT L3 TURBO].)(See BONNET REMOVAL/INSTALLATION [L3 TURBO].)

2. Remove the windshield washer hose from the windshield washer nozzle.

3. Compress the hooks of the windshield washer nozzle.

4. Pull the windshield washer nozzle out to remove it.

5. Install in the reverse order of removal.