#
EGR PIPE REMOVAL/INSTALLATION [L3 Turbo]

id0116b4803800

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF, L3, L3 Turbo].)

2. Remove the battery and battery tray. (See BATTERY REMOVAL/INSTALLATION [L8, LF, L3, L3 Turbo].)

3. Remove the following parts. (See INTAKE AIR SYSTEM REMOVAL/INSTALLATION [L3 Turbo].)

  • Air cleaner
  • Charge air cooler
  • Air hose
  • Air duct

4. Set the throttle body out of the way. (See INTAKE AIR SYSTEM REMOVAL/INSTALLATION [L3 Turbo].)

5. Remove the EGR pipe.

6. Install in the reverse order of removal.