#
AFTER REPAIR PROCEDURE [FS5A-EL]

id050221800400

Caution

• After repairing a malfunction, perform the following procedure to verify that the malfunction has been corrected.

• When performing this procedure, be sure to drive the vehicle at lawful speed and pay attention to the other vehicles.

1. Connect the WDS or equivalent to the DLC-2.

2. Turn the ignition switch to the ON position (engine off).

3. Verify that DTCs are cleared from memory.

4. Perform the following DTC inspections to ensure that the DTCs have been resolved:

DTC No. | inspection
--- | ---
P0706, P0707, P0708 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle in D range at 20 km/h {12.4 mph} or more for 100 s or more. iv. Turn the ignition switch to the LOCK position. v. Start the engine. vi. Drive the vehicle in D range at 20 km/h {12.4 mph} or more for 100 s or more. vii. Go to Step 5.
P0711 | i. Start the engine then wait 180 s or more. ii. Warm up the engine and ATX. iii. Drive the vehicle in D range, at within 25-59 km/h {16-36 mph} for 90 s or more. iv. Drive the vehicle in D range, at 60 km/h {37 mph} for 60 s or more. v. Turn the ignition switch to the LOCK position. vi. Start the engine. vii. Drive the vehicle in D range, at within 25-59 km/h {16-36 mph} for 90 s or more. viii. Drive the vehicle in D range, at 60 km/h {37 mph} or more for 60 s or more. ix. Go to Step 5.
P0712, P0713 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle in D range, at 20 km/h {12 mph} or more for 150 s or more. iv. Go to Step 5.
P0715 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle in D range, at 41 km/h {25 mph} or more for 0.7 s or more. iv. Go to Step 5.
P0720 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle under the following conditions for 4.5 s or more. • Turbine speed (TSS PID): 1,500 rpm or more • Selector lever position: D range, 1GR iv. Turn the ignition switch to the LOCK position. v. Start the engine. vi. Drive the vehicle under the following conditions for 4.5 s or more. • Turbine speed (TSS PID): 1,500 rpm or more • Selector lever position: D range, 1GR vii. Go to Step 5.
P0731 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle under the following conditions 4 times or more. • Turbine speed (TSS PID): 225-4,987 rpm • Selector lever position: D or M range, 1GR • Throttle opening angle (THOP PID): 4.14% or more iv. Go to Step 5.
P0732 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle under the following conditions 3 times or more. • Turbine speed (TSS PID): 225-4,987 rpm • Selector lever position: D or M range, 2GR iv. Go to Step 5.
P0733 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle under the following conditions. • Turbine speed (TSS PID): 225-4,987 rpm • Selector lever position: D or M range, 3GR iv. Go to Step 5.
P0734 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle under the following conditions. • Vehicle speed (VSS PID): 28 km/h {17 mph} or more • Turbine speed (TSS PID): 225-4,987 rpm • Selector lever position: D or M range, 4GR iv. Go to Step 5.
P0735 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle under the following conditions. • Turbine speed (TSS PID): 225-4,987 rpm • Throttle opening angle (THOP PID): 4.14% or more • Selector lever position: D or M range, from 1GR to 5GR iv. Go to Step 5.
P0741 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle under the following conditions for 5 s or more. • Vehicle speed (VSS PID): 60-100 km/h {38-62 mph} • Turbine speed (TSS PID): 225-4,987 rpm • Selector lever position: D range, 4GR iv. Go to Step 5.
P0742 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle under the following conditions. • Vehicle speed (VSS PID): 70 km/h {43 mph} or less • Turbine speed (TSS PID): 225-4,987 rpm • Selector lever position: D range, 4GR • Throttle conditions - Throttle opening angle (THOP PID) is 6.25% or more and 5 s or more have passed. - Throttle opening angle (THOP PID) is within 3.13-6.25% and 3 s or more have passed. - Throttle opening angle is at closed throttle position and 5 s or more have passed. iv. Go to Step 5.
P0744, P0753, P0758, P0763, P0768, P0773, P0778, P0841, P1783, P2709 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle in D range and make sure that the gears shift smoothly from 1GR to 5GR and TCC is operated. iv. Turn the ignition switch to the LOCK position. v. Start the engine. vi. Drive the vehicle in D range and make sure that the gears shift smoothly from 1GR to 5GR and TCC is operated. vii. Go to Step 5.
P0745 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle in D range. iv. Go to Step 5.
P0751 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle under the following conditions for 15 s or more. • Vehicle speed (VSS PID): 36 km/h {22 mph} or more • Turbine speed (TSS PID): 225-4,987 rpm • Selector lever position: D range, 4GR iv. Turn the ignition switch to the LOCK position. v. Start the engine. vi. Drive the vehicle under the following conditions for 15 s or more. • Vehicle speed (VSS PID): 36 km/h {22 mph} or more • Turbine speed (TSS PID): 225-4,987 rpm • Selector lever position: D range, 4GR vii. Go to Step 5.
P0752 | i. Start the engine. ii. Warm up the engine and ATX. iii. Selector lever position: D range iv. Depress the brake pedal. v. Turn the ignition switch to the LOCK position. vi. Start the engine. vii. Selector lever position: D range viii. Depress the brake pedal. ix. Go to Step 5.
P0756 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle under the following conditions 4 times or more. • Turbine speed (TSS PID): 225-4,987 rpm • Throttle opening angle (THOP PID): 4.14% or more • Differential gear case (output) revolution speed (OSS PID): 35 rpm or more • Selector lever position: D range, 1GR iv. Turn the ignition switch to the LOCK position. v. Start the engine. vi. Drive the vehicle under the following conditions 4 times or more. • Turbine speed (TSS PID): 225-4,987 rpm • Throttle opening angle (THOP PID): 4.14% or more • Differential gear case (output) revolution speed (OSS PID): 35 rpm or more • Selector lever position: D range, 1GR vii. Go to Step 5.
P0757, P0766 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle under the following conditions. • Vehicle speed (VSS PID): 28 km/h {17 mph} or more • Turbine speed (TSS PID): 225-4,987 rpm • Throttle opening angle at closed throttle position • Differential gear case (output) revolution speed (OSS PID): 35 rpm or more • Selector lever position: D range, 2GR and 4GR iv. Turn the ignition switch to the LOCK position. v. Start the engine. vi. Drive the vehicle under the following conditions. • Vehicle speed (VSS PID): 28 km/h {17 mph} or more • Turbine speed (TSS PID): 225-4,987 rpm • Throttle opening angle at closed throttle position • Differential gear case (output) revolution speed (OSS PID): 35 rpm or more • Selector lever position: D range, 2GR and 4GR vii. Go to Step 5.
P0761 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle under the following conditions 4 times or more. • Turbine speed (TSS PID): 225-4,987 rpm • Throttle opening angle (THOP PID): 4.14% or more • Differential gear case (output) revolution speed (OSS PID): 35 rpm or more • Selector lever position: D range, 1GR and 2GR iv. Turn the ignition switch to the LOCK position. v. Start the engine. vi. Drive the vehicle under the following conditions 4 times or more. • Turbine speed (TSS PID): 225-4,987 rpm • Throttle opening angle (THOP PID): 4.14% or more • Differential gear case (output) revolution speed (OSS PID): 35 rpm or more • Selector lever position: D range, 1GR and 2GR vii. Go to Step 5.
P0762 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle under the following conditions. • Vehicle speed (VSS PID): 26 km/h {16 mph} or more • Turbine speed (TSS PID): 225-4,987 rpm • Differential gear case (output) revolution speed (OSS PID): 35 rpm or more • Selector lever position: D range, 3GR iv. Turn the ignition switch to the LOCK position. v. Start the engine. vi. Drive the vehicle under the following conditions. • Vehicle speed (VSS PID): 26 km/h {16 mph} or more • Turbine speed (TSS PID): 225-4,987 rpm • Differential gear case (output) revolution speed (OSS PID): 35 rpm or more • Selector lever position: D range, 3GR vii. Go to Step 5.
P0767 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle under the following conditions for 5 s or more. • Turbine speed (TSS PID): 225-4,987 rpm • Selector lever position: D range, 3GR iv. Turn the ignition switch to the LOCK position. v. Start the engine. vi. Drive the vehicle under the following conditions for 5 s or more. • Turbine speed (TSS PID): 225-4,987 rpm • Selector lever position: D range, 3GR vii. Go to Step 5.
P0771 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle under the following conditions for 5 s or more. • Vehicle speed (VSS PID): 60-100 km/h {38-62 mph} • Turbine speed (TSS PID): 225-4,987 rpm • Selector lever position: D range, 4GR iv. Turn the ignition switch to the LOCK position. v. Start the engine. vi. Drive the vehicle under the following conditions for 5 s or more. • Vehicle speed (VSS PID): 60-100 km/h {38-62 mph} • Turbine speed (TSS PID): 225-4,987 rpm • Selector lever position: D range, 4GR vii. Go to Step 5.
P0772 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle under the following conditions. • Vehicle speed (VSS PID): 70 km/h {43 mph} or less • Turbine speed (TSS PID): 225-4,987 rpm • Selector lever position: D range, 4GR • Throttle conditions - Throttle opening angle (THOP PID) is 6.25% or more and 5 s or more have passed. - Throttle opening angle (THOP PID) is within 3.13-6.25% and 3 s or more have passed. - Throttle opening angle is at closed throttle position and 5 s or more have passed. iv. Turn the ignition switch to the LOCK position. v. Start the engine. vi. Drive the vehicle under the following conditions. • Vehicle speed (VSS PID): 70 km/h {43 mph} or less • Turbine speed (TSS PID): 225-4,987 rpm • Selector lever position: D range, 4GR • Throttle conditions - Throttle opening angle (THOP PID) is 6.25% or more and 5 s or more have passed. - Throttle opening angle (THOP PID) is within 3.13-6.25% and 3 s or more have passed. - Throttle opening angle is at closed throttle position and 5 s or more have passed. vii. Go to Step 5.
P0777 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle under the following conditions 4 times or more. • Turbine speed (TSS PID): 225-4,987 rpm • Throttle opening angle (THOP PID): 4.14% or more • Selector lever position: D range, 5GR iv. Turn the ignition switch to the LOCK position. v. Start the engine. vi. Drive the vehicle under the following conditions 4 times or more. • Turbine speed (TSS PID): 225-4,987 rpm • Throttle opening angle (THOP PID): 4.14% or more • Selector lever position: D range, 5GR vii. Go to Step 5.
P0791 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle in D range at 40 km/h {25 mph} or more for 4.5 s or more. iv. Go to Step 5.
P2707 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle under the following conditions 4 times or more. • Turbine speed (TSS PID): 225-4,987 rpm • Throttle opening angle (THOP PID): 4.14% or more • Selector lever position: D range, 3GR or 4GR iv. Turn the ignition switch to the LOCK position. v. Start the engine. vi. Drive the vehicle under the following conditions 4 times or more. • Turbine speed (TSS PID): 225-4,987 rpm • Throttle opening angle (THOP PID): 4.14% or more • Selector lever position: D range, 3GR or 4GR vii. Go to Step 5.
P2708 | i. Start the engine. ii. Warm up the engine and ATX. iii. Drive the vehicle under the following conditions 4 times or more. • Turbine speed (TSS PID): 225-4,987 rpm • Throttle opening angle (THOP PID): 4.14% or more • Selector lever position: D range, 5GR iv. Turn the ignition switch to the LOCK position. v. Start the engine. vi. Drive the vehicle under the following conditions 4 times or more. • Turbine speed (TSS PID): 225-4,987 rpm • Throttle opening angle (THOP PID): 4.14% or more • Selector lever position: D range, 5GR vii. Go to Step 5.
P0894 | i. Start the engine. ii. Warm up the engine and ATX. iii. Depress the brake pedal. iv. Throttle opening angle at closed throttle position. v. Shift the selector lever from the N position to the D range and hold for 3 s or more. vi. Go to Step 6.

5. Gradually slow down and stop the vehicle.

6. Make sure that the repaired DTC does not recur.