#
DTC P2032 [MZR-CD (RF Turbo)]

id0102f1026800

DTC P2032 | Exhaust gas temperature sensor (lower) circuit low input
--- | ---
DETECTION CONDITION | • The PCM monitors the input signal from the exhaust gas temperature sensor (lower). If the voltage from the exhaust gas temperature sensor (lower) is less than 0.24 V, the PCM determines that there is a malfunction in the exhaust gas temperature sensor (lower) circuit. Diagnostic support note • The MIL illuminates if the PCM detects the above malfunction condition in the first drive cycle. • FREEZE FRAME DATA is available. • The DTC is stored in the PCM memory.
POSSIBLE CAUSE | • Exhaust gas temperature sensor (lower) malfunction • Connector or terminal malfunction • Short to ground in wiring harness between exhaust gas temperature sensor (lower) terminal A and PCM terminal 33 • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related service repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | VERIFY CURRENT SIGNAL STATUS: IS CONCERN INTERMITTENT OR CONSTANT? • Connect the WDS or equivalent to the DLC-2. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the same DTC present? | Yes | Go to the next step.
No | Intermittent concern exists. Perform the "INTERMITTENT CONCERN TROUBLESHOOTING". (See INTERMITTENT CONCERN TROUBLESHOOTING [MZR-CD (RF Turbo)].)
4 | INSPECT EXHAUST GAS TEMPERATURE SENSOR (LOWER) CONNECTOR FOR POOR CONNECTION • Turn the engine switch off. • Disconnect the exhaust gas temperature sensor (lower) connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 8.
No | Go to the next step.
5 | INSPECT EXHAUST GAS TEMPERATURE SENSOR (LOWER) SIGNAL CIRCUIT FOR SHORT TO GROUND • Turn the engine switch off. • Inspect for continuity between exhaust gas temperature sensor (lower) terminal A (wiring harness-side) and body ground. • Is there continuity? | Yes | Repair or replace the wiring harness for a possible short to ground, then go to Step 8.
No | Go to the next step.
6 | INSPECT EXHAUST GAS TEMPERATURE SENSOR (LOWER) • Inspect the exhaust gas temperature sensor (lower). (See EXHAUST GAS TEMPERATURE SENSOR INSPECTION [MZR-CD (RF Turbo)].) • Is there any malfunction? | Yes | Replace the exhaust gas temperature sensor (lower), then go to Step 8.
No | Go to the next step.
7 | INSPECT PCM CONNECTOR FOR POOR CONNECTION • Turn the engine switch off. • Disconnect the PCM connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to the next step.
No | Go to the next step.
8 | VERIFY TROUBLESHOOTING OF DTC P2032 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the same DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to the next step.
9 | VERIFY AFTER REPAIR PROCEDURE • Perform the Repair Verification Drive Mode. (See OBD DRIVE MODE [MZR-CD (RF Turbo)].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [MZR-CD (RF Turbo)].)
No | DTC troubleshooting completed.