#
STARTER REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

id0119f1800200

  Warning

  • When the battery cables are connected, touching the vehicle body with starter terminal B will generate sparks. This can cause personal injury, fire, and damage to the electrical components. Always disconnect the negative battery cable before performing the following operation.

1. Disconnect the negative battery cable.

2. Remove the engine cover. (See TIMING BELT REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

3. Remove the air cleaner assembly. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

4. Remove the under cover.

5. Remove the harness bracket with the connector connected. Position the harness bracket so that it is out of the way.

6. Remove in the order indicated in the table.

7. Install in the reverse order of removal.

1 | Terminal B cable
2 | Terminal S connector
3 | Starter