DTC TABLE [AUDIO SYSTEM]

id0902f6837000

Screen display | Detection condition | Possible cause/inspection
--- | --- | ---
DTC (When starting on-board diagnostic test function)
00: Er01 | Cassette deck cannot implement insert and eject commands. | Cassette deck malfunction
00: Er03 | Reel built into cassette deck does not operate. | Verify condition of the cassette deck.
00: Er04 | Cassette tape is worn out. | • Tape wear • Verify condition of the cassette deck.
00: Er10 | Cassette deck does not operate. | • Malfunction of connectors between base unit and cassette deck • Cassette deck malfunction
03: Er01 | CD player cannot implement insert and eject commands. | CD player malfunction
03: Er02 | Cannot change tracks. | CD player malfunction
03: Er07 | CD reading error. | • Defective CD (scratches or dirt) • CD player malfunction
03: Er10 | CD player does not operate. | • Malfunction of connectors between base unit and CD player • CD player malfunction
06: Er01 | CD changer (upper module) cannot implement insert, eject, and disc change commands. | • Defective CD (curved, broken or foreign material stuck/attached, etc.) • CD changer (upper module) malfunction
06: Er02 | Cannot change tracks. | • Defective CD (curved, broken or foreign material stuck/attached, etc.) • CD changer (upper module) malfunction
06: Er07 | CD reading error. | • Defective CD (curved, broken or foreign material stuck/attached, etc.) • CD changer (upper module) malfunction
06: Er10 | CD changer (upper module) does not operate. | • Malfunction of connectors between base unit and CD changer (upper module) • CD changer (upper module) malfunction
07: Er01 | MD player cannot implement insert and eject commands. | MD player malfunction
07: Er02 | Cannot change tracks. | MD player malfunction
07: Er07 | MD reading error. | Defective MD
07: Er08 | Blank unrecorded MD is inserted. | Defective MD
07: Er10 | MD player does not operate. | • Malfunction of connectors between base unit and MD player • MD player malfunction
09: Er20 | Audio system does not operate. | Voltage at base unit is low.
09: Er21 | Broken sound/No sound | • Base unit internal malfunction or base unit protection function operates • Speaker or speaker circuit malfunction
09: Er22 | No radio reception | Inspect the radio operation according to vehicle condition.
10: Er01 | MP3 applicable CD player cannot implement insert and eject commands. | MP3 applicable CD player malfunction
10: Er02 | Cannot change tracks. | MP3 applicable CD player malfunction
10: Er07 | MP3 CD reading error. | Incorrect format CD
10: Er10 | MP3 applicable CD player does not operate. | • Malfunction of connectors between base unit and MP3 applicable CD player • MP3 applicable CD player malfunction
16: Er12 | — | CAN system
17: Er11 | — | CAN system
18: Er11 | — | CAN system
19: Er11 | — | CAN system
19: Er17 | Incorrect combination (base unit and center panel) | Install the correct base unit or the center panel.
19: Er18
19: Er19 | Communication error between base unit and center panel | Malfunction of connectors between base unit and center panel
20: Er01 | CD player cannot implement insert and eject commands. | • Over heat/cool protection function is operating • HDD malfunction
20: Er02 | Cannot change tracks. | • Over heat/cool protection function is operating • HDD malfunction
20: Er07 | CD reading error. | • Defective CD (curved, broken or foreign material stuck/attached, etc.) • HDD malfunction
20: Er10 | CD player/HDD does not operate. | • Over heat/cool protection function is operating • HDD malfunction
20: Er14 | HDD reading error. | • Verify the HDD unit using condition • HDD malfunction
HDD reading error. | HDD malfunction (need of format)
HDD writing error. | • Defective CD (curved, broken or foreign material stuck/attached, etc.) • HDD malfunction
HDD writing error (system file) | • Over heat/cool protection function is operating • Defective CD (curved, broken or foreign material stuck/attached, etc.) • HDD malfunction
HDD writing error (system file) | • Over heat/cool protection function is operating • Defective CD (curved, broken or foreign material stuck/attached, etc.) • HDD malfunction
20: Er15 | Writing stop by low battery voltage | Inspect the battery voltage.
20: Er16 | HDD over heat/cool | Over heat/cool protection function is operating
21: Er19 | Audio system communication error | Center panel malfunction
22: Er01 | MP3 applicable CD changer cannot implement insert, eject, and disc change commands. | • Defective CD (curved, broken or foreign material stuck/attached, etc.) • MP3 applicable CD changer malfunction
22: Er02 | Cannot change tracks. | • Defective CD (curved, broken or foreign material stuck/attached, etc.) • MP3 applicable CD changer malfunction
22: Er07 | CD reading error. | • Defective CD (curved, broken or foreign material stuck/attached, etc.) • MP3 applicable CD changer malfunction
22: Er10 | MP3 applicable CD changer does not operate. | • Malfunction of connectors between base unit and MP3 applicable CD changer • MP3 applicable CD changer malfunction
no Err | No DTCs stored | No DTCs stored