#
DTC TABLE [FS5A-EL]

id050221800500

DTC No. | Condition | MIL | AT warning light illuminates | DC | Monitor item | Memory function | Page
--- | --- | --- | --- | --- | --- | --- | ---
P0706 | Transaxle range (TR) switch circuit range/performance | ON | YES | 2 | CCM | X | (See DTC P0706 [FS5A-EL].)
P0707 | Transaxle range (TR) switch circuit low input | ON | YES | 1 | CCM | X | (See DTC P0707 [FS5A-EL].)
P0708 | Transaxle range (TR) switch circuit high input | ON | YES | 2 | CCM | X | (See DTC P0708 [FS5A-EL].)
P0711 | Transaxle fluid temperature (TFT) sensor circuit range/performance (stuck) | ON | NO | 2 | CCM | X | (See DTC P0711 [FS5A-EL].)
P0712 | Transaxle fluid temperature (TFT) sensor circuit malfunction (short to ground) | ON | YES | 1 | CCM | X | (See DTC P0712 [FS5A-EL].)
P0713 | Transaxle fluid temperature (TFT) sensor circuit malfunction (open circuit) | ON | YES | 1 | CCM | X | (See DTC P0713 [FS5A-EL].)
P0715 | Input/turbine speed sensor circuit malfunction | ON | YES | 1 | CCM | X | (See DTC P0715 [FS5A-EL].)
P0720 | Vehicle speed sensor (VSS) circuit malfunction | ON | YES | 1 | CCM | X | (See DTC P0720 [FS5A-EL].)
P0731 | Gear 1 incorrect (incorrect gear ratio detected) | OFF | YES | 1 | CCM | X | (See DTC P0731 [FS5A-EL].)
P0732 | Gear 2 incorrect (incorrect gear ratio detected) | OFF | YES | 1 | CCM | X | (See DTC P0732 [FS5A-EL].)
P0733 | Gear 3 incorrect (incorrect gear ratio detected) | OFF | YES | 1 | CCM | X | (See DTC P0733 [FS5A-EL].)
P0734 | Gear 4 incorrect (incorrect gear ratio detected) | OFF | YES | 1 | CCM | X | (See DTC P0734 [FS5A-EL].)
P0735 | Gear 5 incorrect (incorrect gear ratio detected) | OFF | YES | 1 | CCM | X | (See DTC P0734 [FS5A-EL].)
P0741 | Torque converter clutch (TCC) (stuck off) | OFF | YES | 1 | CCM | X | (See DTC P0741 [FS5A-EL].)
P0742 | Torque converter clutch (TCC) (stuck on) | OFF | YES | 1 | CCM | X | (See DTC P0742 [FS5A-EL].)
P0744 | Slip control malfunction | OFF | YES | 2 | CCM | X | (See DTC P0744 [FS5A-EL].)
P0745 | Pressure control solenoid A malfunction | OFF | YES | 1 | CCM | X | (See DTC P0745 [FS5A-EL].)
P0751 | Shift solenoid A stuck off | ON | YES | 2 | CCM | X | (See DTC P0751 [FS5A-EL].)
P0752 | Shift solenoid A stuck on | ON | YES | 2 | CCM | X | (See DTC P0752 [FS5A-EL].)
P0753 | Shift solenoid A malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P0753 [FS5A-EL].)
P0756 | Shift solenoid B stuck off | ON | YES | 2 | CCM | X | (See DTC P0756 [FS5A-EL].)
P0757 | Shift solenoid B stuck on | ON | YES | 2 | CCM | X | (See DTC P0757 [FS5A-EL].)
P0758 | Shift solenoid B malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P0758 [FS5A-EL].)
P0761 | Shift solenoid C stuck off | ON | YES | 2 | CCM | X | (See DTC P0761 [FS5A-EL].)
P0762 | Shift solenoid C stuck on | ON | YES | 2 | CCM | X | (See DTC P0762 [FS5A-EL].)
P0763 | Shift solenoid C malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P0763 [FS5A-EL].)
P0766 | Shift solenoid D stuck off | ON | YES | 2 | CCM | X | (See DTC P0766 [FS5A-EL].)
P0767 | Shift solenoid D stuck on | ON | YES | 2 | CCM | X | (See DTC P0767 [FS5A-EL].)
P0768 | Shift solenoid D malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P0768 [FS5A-EL].)
P0771 | Shift solenoid E stuck off | ON | YES | 2 | CCM | X | (See DTC P0771 [FS5A-EL].)
P0772 | Shift solenoid E stuck on | ON | YES | 2 | CCM | X | (See DTC P0772 [FS5A-EL].)
P0773 | Shift solenoid E malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P0773 [FS5A-EL].)
P0777 | Pressure control solenoid B stuck on | ON | YES | 2 | CCM | X | (See DTC P0777 [FS5A-EL].)
P0778 | Pressure control solenoid B malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P0778 [FS5A-EL].)
P0791 | Intermediate sensor circuit malfunction | ON | YES | 1 | CCM | X | (See DTC P0791 [FS5A-EL].)
P0841 | Oil pressure switch circuit malfunction | OFF | NO | 2 | CCM | X | (See DTC P0841 [FS5A-EL].)
P0882 | Battery back-up power supply circuit malfunction | ON | NO | 1 | CCM | X | (See DTC P0882 [FS5A-EL].)
P0894 | Forward clutch torque transmission | OFF | YES | 1 | CCM | X | (See DTC P0894 [FS5A-EL].)
P1783 | ATF high oil temperature malfunction | OFF | YES | 1 | CCM | X | (See DTC P1783 [FS5A-EL].)
P2707 | Shift solenoid F stuck off | ON | YES | 2 | CCM | X | (See DTC P2707 [FS5A-EL].)
P2708 | Shift solenoid F stuck on | ON | YES | 2 | CCM | X | (See DTC P2708 [FS5A-EL].)
P2709 | Shift solenoid F malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P2709 [FS5A-EL].)
U0073 | CAN system communication error | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0100 | Communication error to PCM | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])