#
TRANSFER REMOVAL/INSTALLATION [JA5AX-EL]

id031611800600

1. Disconnect the negative battery cable.

2. Remove the propeller shaft. (See PROPELLER SHAFT REMOVAL/INSTALLATION [JA5AX-EL].)

3. Remove the TWC. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L3 4WD].)

4. Remove the front tires and splash shield of right side.

5. Remove the under cover.

6. Remove the drive shaft of right side. (See FRONT DRIVE SHAFT REMOVAL/INSTALLATION [L8, LF, L3, MZR-CD (RF Turbo)].)

7. Remove the joint shaft. (See JOINT SHAFT REMOVAL/INSTALLATION [L8, LF, L3, MZR-CD (RF Turbo)].)

8. Remove the exhaust manifold insulator. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L3 4WD].)

9. Remove the exhaust manifold. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L3 4WD].)

10. Remove in the order shown in the figure.

1 | No.1 engine mount installation bolt (See No.1 Engine Mount Installation Bolt Removal Note.) (See No.1 Engine Mount Installation Bolt Installation Note.)
2 | PTO heat shield (See PTO Heat Shield Installation Note.)
3 | Transfer

11. Install in the reverse order of removal.

## No.1 Engine Mount Installation Bolt Removal Note

1. Loosen the bolt A.

2. Remove the bolt B.

3. Remove the bolt C and D.

## No.1 Engine Mount Installation Bolt Installation Note

1. Tighten the bolt C and D.

2. Lightly tighten the bolt B, then bolt A.

3. Tighten the bolt B and A.

Tightening torque

  A, C, D: 93.1-116.6 N·m
  {9.50-11.88 kgf·m, 68.66-85.98 ft·lbf}
  B: 85.3-116.6 N·m
  {8.70-11.88 kgf·m, 62.91-85.98 ft·lbf}

## PTO Heat Shield Installation Note

1. Lightly tighten the bolt A.

2. Tighten the bolt B, then bolt C.

3. Tighten the bolt A.

Tightening torque

  8-11 N·m
  {82-112 kgf·cm, 72-97 in·lbf}