#
AUTOMATIC TRANSAXLE DEVICE RELATIONSHIP CHART [JA5AX-EL]

id051705250800

Component | Control item
--- | ---
Shift control | Line pressure control | Reverse inhibition control | Shift transient control | Feedback control | TCC control | N-D select control | Slope mode control | OBD system
Input
TR switch | X | X | X | X | X | X | X |  | X
Input/turbine speed sensor |  | X |  | X | X | X | X | X | X
Intermediate sensor |  | X |  | X | X |  |  |  | X
Vehicle speedometer sensor | X | X | X | X | X | X | X | X | X
TFT sensor | X | X |  | X | X | X | X |  | X
Brake switch | X |  |  |  |  | X |  | X |
M range switch | X |  |  |  |  | X |  |  |
Up switch | X |  |  |  |  | X |  |  |
Down switch | X |  |  |  |  | X |  |  |
CAN signal | Throttle position signal | X | X |  | X | X | X | X | X | X
Engine torque signal (without torque down) |  | X |  | X | X |  | X | X | X
Engine torque signal (with torque down) |  | X |  | X | X |  | X |  | X
Engine torque signal (loss torque) |  | X |  | X | X |  | X | X | X
Engine coolant temperature signal | X |  |  |  |  |  |  |  | X
Engine speed signal | X |  |  | X | X | X |  | X | X
Torque reduce signal |  | X |  | X | X |  | X |  | X
Battery OFF signal |  |  |  |  | X |  |  |  | X
Output
ON/OFF type | Shift solenoid A | X |  |  | X |  |  |  |  | X
Shift solenoid B | X |  |  | X |  |  |  |  | X
Shift solenoid C | X |  |  | X |  |  |  |  | X
Reduction timing solenoid valve |  | X |  | X |  |  |  |  | X
Neutral shift solenoid valve | X | X | X | X |  |  |  |  | X
Duty type | Pressure control solenoid | X | X |  | X | X |  |  |  | X
2-4 brake solenoid valve | X | X |  | X | X |  |  |  | X
High clutch solenoid valve | X | X |  | X | X |  |  |  | X
TCC solenoid valve |  | X |  |  |  | X |  |  | X
CAN signal | Reduce torque signal |  |  |  |  | X |  | X |  | X
Range signal |  |  |  |  |  |  |  |  | X
Turbine speed signal |  |  |  |  |  |  |  |  | X
ATF temperature signal |  |  |  |  |  |  |  |  | X
TCC signal |  |  |  |  |  | X |  |  | X
Racing select signal |  |  |  |  |  |  |  |  | X
MIL indicate request signal |  |  |  |  |  |  |  |  | X
AT warning light request signal |  |  |  |  |  |  |  |  | X

  X :
Available