#
NO.3 VEHICLE MOVES IN P POSITION, OR PARKING GEAR DOES NOT DISENGAGE WHEN P IS DISENGAGED [JA5AX-EL]

id050305800800

3 | Vehicle moves in P position, or parking gear does not disengage when P is disengaged
DESCRIPTION | • Vehicle rolls when on a downward slope and tires do not lock in P position. • Tires locked when P disengaged, vehicle does not move in D range, and R position when accelerator pedal depressed, and engine remains in stall condition.
POSSIBLE CAUSE | • Malfunction of parking mechanism (May have effect on noise or shock from transaxle) • Improper adjustment of selector lever • If vehicle moves in N position, perform symptom troubleshooting No.2 "Vehicle moves in N position" Note • Before following troubleshooting steps, make sure that Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.