#
FUEL-FILLER LID AND OPENER REMOVAL/INSTALLATION

id091000405000

1. To remove the fuel-filler lid opener, remove the left side trunk side trim (4SD) or trunk side lower trim (5HB, WGN).

2. To remove the fuel-filler lid opener cable, perform the following and turn over the floor covering.

  (1) Remove the driver-side front seat.
  (2) Remove the driver-side front scuff plate.
  (3) Remove the driver-side rear scuff plate.
  (4) Remove the driver-side B-pillar lower trim.
  (5) Remove the driver-side tire house trim.
  (6) Remove the rear seat cushion. (R.H.D., 4SD, WGN (4WD))
  (7) Remove the rear seat installation bolts (front side), then lift the rear seat cushion. (R.H.D., 5HB, WGN (2WD))

3. Remove in the order indicated in the table.

1 | Fuel-filler lid
2 | Lift spring
3 | Fuel-filler lid opener
4 | Cover
5 | Fuel-filler lid opener lever
6 | Fuel-filler lid opener cable

4. Install in the reverse order of removal.

5. Adjust the fuel-filler lid. (See FUEL-FILLER LID ADJUSTMENT.)